 +---------------------------------------------------------------------------+
                         *-*-*   READ.ME   *-*-*

 This file contains a description of the iRMX III Multibus II System Parameter
 Strings (SPS parameters).  These parameters can be entered on the Master Test
 Handler command line or can be placed in the BPS File which is read by the
 MSA BootServer during iRMX initialization.  The name of the iRMX feature
 affected by the parameters is preceded by a double asterix.  The Major SPS
 parameter is preceded by a dash and any Minor SPS parameters are then
 described.  Remember that Board Names are case sensitive.

 Refer to the MSA for the System 520 manual for more details.
 +---------------------------------------------------------------------------+


** System Device

 - RQ_SD - iRMX physical device name or remote device of System Device.


** PCI Driver

 - RQ_PCI_x:
   Board Name (BNAM)     - Multibus II Board Name found in interconnect space.
   Board Instance (BIN)  - instance of server host with the specified Board
                           Name starting with the one in lowest numbered slot.
   Server Instance (SIN) - instance of server on the server host.


** ATCS Driver

 - RQ_ATCS_xxx:
   Board Name (BNAM)    - Multibus II Board Name found in interconnect space.
   Board Instance (BIN) - instance of server host with the specified Board
                          Name starting with the one in lowest numbered slot.
   Slot ID (SID)        - Multibus II slot number containing the server host.


** Multibus II Downloader

 - RQ_DLJ:
   iRMX Device Name (DEV) - physical device name of the storage device
                            containing the downloader configuration file.
   File Driver (FDVR)     - file driver (named, remote) for the storage device
                            specified by the DEV parameter.


** iRMX-NET

 - RQ_MIP:
   Board Name (BNAM)      - Multibus II Board Name found in interconnect space.
   Board Instance (BIN)   - instance of Ethernet controller with the specified
                            Board Name starting with the one in lowest
                            numbered slot.
   File Name (FILE)       - path name of the the iNA download file.
   iRMX Device Name (DEV) - physical device name of the storage device
                            containing the iNA download file.
   Load Method (LOAD)     - method in which the COMMengine is loaded.
                            (local, remote, noload, prom)
   Class Code (CC)        - class code that the COMMengine uses when requesting
                            loading over the network.


** iNA MIP Driver

 - RQ_MIP_xx:
   (xx indicates the instance of the iNA server, valid values are 00-19)
   Board Name (BNAM)      - Multibus II Board Name found in interconnect space.
   File Name (FILE)       - path name of the the iNA download file.
   iRMX Device Name (DEV) - physical device name of the storage device
                            containing the iNA download file.
   Load Method (LOAD)     - method in which the COMMengine is loaded.
                            (local, remote, noload, prom)
   Class Code (CC)        - class code that the COMMengine uses when requesting
                            loading over the network.
 +---------------------------------------------------------------------------+
