#
#   *-*-*   BPS.RMX   *-*-*
#
#   iRMX III MSA Bootstrap Parameter String configuration file for use on
#   Multibus II Microcomputers when:
#      1) an iSBC 486/133SE board boots Independently from its local
#         SCSI I/O subsystem using the default I/O controller boot file
#         pathname /msa32/boot/rmxio and executes in an I/O controller-only
#         mode.
#      2) a single CPU board boots Quasi-independently from that
#         iSBC 486/133SE board using the default Multibus II boot file
#         pathname /msa32/boot/rmx.
#
#   Refer to /msa32/read.me for a description of the BPS and SPS parameters.

#   The iSBC 486/133SE must be in slot 0; the QI-master CPU must be in slot 2.
#   BPS Parameters for an iSBC 486/133SE board booting Independently.

[bl_host_id = 0]
	bl_target_file = /msa32/boot/rmxio;
	bl_qi_master = 2

#   BPS Parameters for a CPU board booting Quasi-independently in slot 2.

[bl_host_id = 2;
	bl_method = quasi]
	bl_target_file = /msa32/boot/rmx;
	rq_pci_a = bnam:486/133SE,bin:1,sin:0;
	rq_atcs_con = bnam:486/133SE,bin:1;
	rq_atcs_a = bnam:186/410,bin:1;
	rq_atcs_b = bnam:186/450,bin:1;
	rq_atcs_c = bnam:MIX386/020,bin:1;
	rq_atcs_d = bnam:386/120,bin:0,sid:31;
	rq_dlj = dev:SCW_2,fdvr:named;
	rq_mip = bnam:486/133SE,bin:1,load:noload;
	rq_sd = SCW_2
